i.MX 6 Series Platform SDK

Version D

# Introduction

The purposes of the Platform SDK for the i.MX 6 Series are to:

* Provide easily understood driver code that supports the primary features of a peripheral.
* Demonstrate key use cases of the chips.
* Provide unit tests for drivers to demonstrate their main features.
* Provide a simple environment for quick board validation and bring-up.
* Provide a source of entirely non-GPL example driver code.
* Includes consistent, documented register access macros for all hardware IP blocks.
* Uses the IOMUX Tool to generate mux configuration code.
* Provides register definitions for ARM RealView Debugger and Lauterbach TRACE32.

The result is an SDK that provides reusable system code and a large number of drivers with related unit tests. For board bring-up, each module can be individually tested one at a time rather than having to bring up most drives all at once. Based on a common initialization of the i.MX6 and the development board, a test for a specific peripheral is launched with the help of a serial console for human interaction.

Also included in the release package are a Firmware Guide (iMX6FG\_RevD.pdf) and IOMUX Tool application (IOMux.exe).

# Versions Available

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Version** | **Release Date** | **Description** |
| SDK Software | D | 29-Jun-2012 | Release with complete driver set. |
| Firmware Guide | D | 29-Jun-2012 | Detailed driver documentation and use guide for chip peripherals. |
| IOMUX Tool | 3.3.2.1 | 29-Jun-2012 | IOMUX configuration tool Windows application |

# Source code structure of the library

|  |  |
| --- | --- |
| **Description** | **Location** |
| Configuration files used to enable features supported by a board. e.g., mx6dq\_sabre\_lite.conf | ./configs |
| SDK documentation files. Doxygen output appears in an html child directory. | ./doc |
| Non-driver shared components. | ./sdk/common |
| Source code related to the ARM Cortex-A9 MPCore platform. | ./sdk/cortex\_a9 |
| Common headers which are chip and board independent. | ./sdk/include |
| Headers specific to the i.MX6 series. | ./sdk/include/mx6dq  ./sdk/include/mx6sdl |
| Generated register headers. | ./sdk/include/mx6dq/registers  ./sdk/include/mx6sdl/registers |
| Global library source file such main, system initialization. | ./sdk/init |
| Source code specific to the i.MX6 series. | ./sdk/mx6dq/  ./sdk/mx6sdl/ |
| IOMUX Tool board design files and generated code directories. | ./sdk/mx6dq/*<board>*/  ./sdk/mx6sdl/*<board>*/ |
| Parent directory for all drivers, includes, and their unit tests and docs. | ./sdk/drivers/ |
| Miscellaneous utility components. | ./sdk/utility |
| Build script and utilities. | ./tools |
| ARM RealView Debugger BCD files | ./tools/rvd/registers |
| Lauterbach TRACE32 peripheral files | ./tools/lauterbach |

Example for a driver:

|  |  |
| --- | --- |
| **Description** | **Location** |
| TEMPMON driver source code. | ./sdk/drivers/tempmon/src/ |
| TEMPMON driver public includes. | ./sdk/drivers/tempmon/tempmon.h |
| TEMPMON driver unit tests. | ./sdk/drivers/tempmon/test/ |

# System requirements

To build the Platform SDK, either a Linux host or Windows host with Cygwin installed may be used.

## Working with Cygwin

Cygwin can be installed and obtained from here:

<http://www.cygwin.com/>

The installation procedure is documented on this site. Some standard packages are necessary, such as make, bash, and perl, but that list is not thorough.

The cygpath program is a utility that converts Windows native filenames to Cygwin POSIX-style pathnames and vice versa. It can be used when a Cygwin program needs to pass a file name to a native Windows program, or expects to get a file name from a native Windows program.

When using the CodeBench toolchain (see below), it is necessary to set this environment variable (sh syntax, csh will use a different syntax):

export CYGPATH=cygpath

**Note:** Version 3.81 of the make package in Cygwin might cause build failures due to a known problem with that version related to correctly handling Windows pathnames. To avoid this issue, it is recommended to verify that make version 3.82 or later is being used. 3.82 is the default version for new installations and upgrades of Cygwin as of this writing.

## Installing the toolchain

The SDK is built using the Mentor Sourcery CodeBench Lite (previously called Sourcery G++ Lite) version of the arm-none-eabi GCC toolchain. The latest version as of this writing is 4.6.3, obtained here:

<https://sourcery.mentor.com/GNUToolchain/release2188>

Versions that are known to work with the SDK are as follows:

|  |  |  |
| --- | --- | --- |
| **Package** | **gcc version** | **Date** |
| [Sourcery CodeBench Lite 2012.03-56](https://sourcery.mentor.com/GNUToolchain/release2188) | 4.6.3 | 2012-06-11 |
| [Sourcery CodeBench Lite 2011.09-69](https://sourcery.mentor.com/GNUToolchain/release2032) | 4.6.1 | 2011-12-19 |
| [Sourcery G++ Lite 2011.03-42](https://sourcery.mentor.com/GNUToolchain/release1802) | 4.5.2 | 2011-05-02 |

The full list of CodeBench Lite releases is available on this page:

<https://sourcery.mentor.com/GNUToolchain/subscription3053?lite=arm&lite=ARM>

Download either the Windows or Linux installer package. The tarball packages do not include all executables.

Install the package under /opt or any other local folder, and make sure that the PATH environment variable allows accessing these executables used for the build process:

CC = arm-none-eabi-gcc

CXX = arm-none-eabi-g++

AS = arm-none-eabi-as

AR = arm-none-eabi-ar

LN = arm-none-eabi-ld

Example (sh syntax):

export PATH=$PATH:*<toolchain\_install\_path>*/bin

Otherwise, it is possible to redefine the above list in the file ./*<sdk\_install\_path>*/make.def with the complete path to the executable.

## Source code installation

The SDK source code package can be installed anywhere.

It is not recommended to use a Windows unzip program to extract the sources, as this may result in line endings being automatically converted. Instead, the equivalent command of Cygwin or Linux should be used.

Example:

tar zxvf mx6series\_sdk\_release.tar.gz

## Build command

To build the SDK, use the ./tools/build\_sdk command.

**Note:** It is important to run build\_sdk from the SDK root directory, not from within the tools directory.

The detailed usage that is printed for the -help option is as follows:

Usage:

build\_sdk [-t <target>] [-b <board>] [-v <rev>] [-r <test>] [-n] [-c] [-l]

Generates makefiles for the i.MX SDK project.

Options:

-t, -target=<target> Specify the target name. Optional, and the default is all.

-b, -board=<brd> Specify the board name. Optional, and the default is all.

-v, -board\_rev=<rev> Specify the board revision. Optional, and the default is all.

-r, -test=<name> Optional argument to select a single test, or ALL for all tests. Defaults to ALL.

-c, -clean Optional flag to force a clean build.

-n, -no-build Don't actually run make.

-l, -list-builds Optional flag to list target, board, board\_rev cominations to be built.

Short options take the same arguments as their respective long options.

The '=' is optional for long options; arguments can be specified as -arg=value or

-arg value. Short options require a space between the option and value.

Generates makefiles for the specified combination of options. If -clean was specified,

'make clean' will be run. Then a regular build will be executed, unless the -no-build

argument is present. Makefiles are generated only for packages that are part of the

selected board.

Valid target and board combinations:

target=mx6dq boards:

sabre\_ai rev a, b

evb rev a (MX6QCPUDDR3)

smart\_device rev a, b

sabre\_lite rev a, b, c

target=mx6sdl boards:

sabre\_ai rev a, b

evb rev a (MX6QCPUDDR3)

smart\_device rev a, b

target=all

builds all valid combinations of target, board, and board\_rev

[-r <test>] is a valid option.

-clean Only does clean builds.

Examples:

build\_sdk -target mx6dq -board evb

Build for the mx6dq evb board with default board rev a, and all tests.

build\_sdk -t mx6dq -b sabre\_ai -v a -test sdma -clean

Build the mx6dq sabre\_ai board with explicit board rev a, but only build the sdma test.

Clean before building.

build\_sdk -target=mx6dq -board=evb -test=gpmi -no-build

Generate the makefiles for mx6dq evb and the gpmi test, but don't actually run make.

build\_sdk -target=all -test vpu

Clean build of vpu\_test for all valid combinations of target, board, and board\_rev.

Running build\_sdk will automatically generate makefiles for every directory listed in the .conf file (in the configs directory) associated with the select target and board. A root level makefile will also be created.However, this makefile cannot be used to build the SDK. The build\_sdk script must always be used to start a build.

The set of boards and revisions supported by this SDK release are listed here:

|  |  |  |
| --- | --- | --- |
| **Name** | **Description** | **Revisions** |
| evb | Freescale validation board, labeled MX6QCPUDDR3 | A only |
| sabre\_ai | Automotive reference design | A, B |
| sabre\_lite | General purpose reference design | A, B, C |
| smart\_device | Smart device reference design | A, B |

The listed tests below are not available for all boards. This is usually due to lack of components or connectors on the given board.

Available tests:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Module** | **Test Name** | **Board1** | | | |
| **evb** | **sabre\_ai** | **sabre\_lite** | **smart\_device** |
| Audio, SSI and audiomux | audio | ✓ | ✓ | ✓ | ✓ |
| Camera | camera | - | - | - | ✓ |
| CAN | flexcan | - | ✓ | - | - |
| cpu\_utility | cpu\_get\_cores | ✓ | ✓ | ✓ | ✓ |
| ENET for Ethernet | enet | ✓ | - | - | - |
| EPIT | epit | ✓ | ✓ | ✓ | ✓ |
| GIC, multicore startup | gic\_multicore | ✓ | ✓ | ✓ | ✓ |
| GIC, software interrupts | gic\_sgi | ✓ | ✓ | ✓ | ✓ |
| GPMI | gpmi | ✓ | - | - | - |
| GPT | gpt | ✓ | ✓ | ✓ | ✓ |
| GPU | gpu | ✓ | - | - | - |
| HDMI | hdmi | ✓ | ✓ | ✓ | ✓ |
| I2C | i2c | ✓ | ✓ | ✓ | ✓ |
| IPU for display | ipu | ✓ | ✓ | ✓ | ✓ |
| LDB for LVDS display | ipu | ✓ | ✓ | ✓ | ✓ |
| KEYPAD | kpp | ✓ | - | - | - |
| MIPI | mipi | ✓ | ✓ | - | - |
| OCOTP for e-fuses | ocotp | ✓ | ✓ | ✓ | ✓ |
| Low power modes | power\_modes | ✓ | ✓ | ✓ | ✓ |
| PCIe | pcie | ✓ | - | - | - |
| PMU | pmu | ✓ | ✓ | ✓ | ✓ |
| PWM | pwm | ✓ | - | - | - |
| SATA for Hard Drive | sata | ✓ | ✓ | ✓ | ✓ |
| SDMA | sdma | ✓ | ✓ | ✓ | ✓ |
| SNVS RTC | snvs\_rtc | ✓ | ✓ | ✓ | ✓ |
| SNVS SRTC | snvs\_srtc | ✓ | ✓ | ✓ | ✓ |
| SPI | spi | ✓ | - | - | - |
| Timer | microseconds | ✓ | ✓ | ✓ | ✓ |
| TEMPMON | tempmon | ✓ | ✓ | ✓ | ✓ |
| UART | uart | ✓ | ✓ | ✓ | ✓ |
| USB | usb | - | ✓ | - | - |
| USDHC for SD/MMC | usdhc | ✓ | ✓ | ✓ | ✓ |
| Video decoder | vpu | ✓ | - | ✓ | ✓ |
| Watchdog | wdog | ✓ | ✓ | ✓ | ✓ |
| WEIM | weim | ✓ | ✓ | - | - |
| ALL | ALL2 | ✓ | ✓ | ✓ | ✓ |

1 ‘✓’ indicates that all boards revisions are supported, otherwise the supported revision is specified.

2 The option ALL includes all tests with the possibility to run, re-run, or skip some of tests.

Once the build is finished a completion message will be printed showing where the ELF output file is located. The build produces an ELF file, a binary image, and a map file. Output files can be found in:

./output/*<cpu>*/*<board>*\_rev\_*<rev>*/bin/

The output file name contains the targeted CPU, board, board revision, and the name of the chosen test.

Example output files in the bin directory:

mx6dq\_sabre\_ai\_rev\_a-vpu-sdk.elf

mx6dq\_sabre\_ai\_rev\_a-vpu-sdk.bin

mx6dq\_sabre\_ai\_rev\_a-vpu-sdk.map

Example build completion message:

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Build has completed. ELF file available at:

=> /home/creed/diag-sdk/output/mx6sdl/evb\_rev\_b/bin/mx6sdl\_evb\_rev\_b-ALL-sdk.elf

Build mx6sdl evb rev\_b ALL passed!

Adding the option -clean to the build\_sdk command line will remove the CPU output directory found under ./output prior to building. Example:

./tools/build\_sdk -t mx6dq -b sabre\_ai -v a -test sdma -clean

# How to run a test

## Setup required

An i.MX 6Dual/6Quad or i.MX 6Solo/6DualLite board is necessary to run a test. Please refer to the appropriate board user guide to prepare this setup.

The user interaction and output information are available through the serial port UART4 connected to a host running terminal software such TeraTerm, minicom, HyperTerminal, or a similar program.

The configuration for the terminal is common: 115200 bps 8N1 (8 data bits, no parity, 1 stop bit).

## Download with a JTAG probe

The code can be downloaded and executed through any JTAG tool that supports the Cortex-A9.

It is necessary to have a board initialization file that will initialize some of the clocks, the MMDC controller and its interface, as well as the DDR3.

The SDK package contains a debugger initialization script for the ARM RealView Debugger:

./tools/rvd/mx6dq\_init.inc

Run this script in the debugger after opening a connection to the i.MX6 Series device. After the script finishes, DDR3 memory is available for use. At this point you can load the ELF output file from the build and run the test.

## Download with the manufacturing tool

The manufacturing tool can be obtained from the Freescale i.MX Design tool web page:

<http://www.freescale.com/webapp/sps/site/overview.jsp?code=IMX_DESIGN>

Below is an example of profile that can be added in the ucl.xml:

<LIST name="DWLD\_IN\_SDP" desc="Download and execute a binary!">

<CMD type="find" body="Recovery" timeout="180"/>

<CMD type="boot" body="Recovery" file="mx6dq\_sabre\_ai\_rev\_a-vpu-sdk.bin">Loading SDK image</CMD>

<CMD type="jump">Jumping to SDK image.</CMD>

</LIST>

## Using SD boot

The SDK binary image can be programmed on a SD card using 2 different methods, depending on the host OS being used.

**Using a Windows host:**

By using the cfimager-imx.exe provided with the release package under folder ./tools/windows.

Use this command:

cfimager-imx.exe –o 0x0 –f ./output/mx6dq/evb\_rev\_a/bin/mx6dq\_evb\_rev\_a-ALL-sdk.bin –d *<your drive letter for the SD card>*

For example, if the drive letter of the SD card reader is F:, type the following:

cfimager-imx.exe –o 0x0 –f ./output/mx6dq/evb\_rev\_a/bin/mx6dq\_evb\_rev\_a-ALL-sdk.bin –d f

There is also the option of formatting the card first before programming it, though be warned it will take more time for this operation to complete due to the card formatting. To invoke the card formatting, simply append the above command with “-a”, as provided in the following example (again, assuming the drive letter is “f”):

cfimager-imx.exe –o 0x0 –f ./output/mx6dq/evb rev\_a/bin/mx6dq\_evb\_rev\_a-ALL-sdk.bin –d f -a

**Using a Linux host:**

Use the command dd under Linux to format the SD card:

dd if=output/mx6dq/evb\_rev\_a/bin/mx6dq\_evb\_rev\_a-ALL-sdk.bin of=/dev/sdx seek=2 skip=2 bs=512 && sync

/dev/sdx is the Linux device for your SD card.

The seek option allows to not change the first 1kB of the SD card where a partition table could reside. The skip option is to remove the unnecessary first 1kB from the binary as the seek option is used.

Once the SD card is programmed successfully with a bootable SDK image, follow below instructions on how to run it on the i.MX6DQ EVB board:

* Insert SD card with SDK binary into SD slot.
* Configure boot dip switches for boot from SD:
  + SW1: off-off-off-off-off-off-ON-off
  + SW2: off-off-off-ON-ON-off-off-off
  + SW5: all off
  + SW8: all off.
* Power on board, and follow on screen prompt commands on host’ terminal window.

# How to add a new driver and test

A new driver should typically be added in a new directory under the ./sdk/drivers/ directory. Public headers go directly into the driver directory root, the source code and private headers into ./sdk/drivers/<new\_driver>/src, and its unit test into ./sdk/new\_driver/test.

In the board config file, such as mx6dq\_evb\_rev\_a.conf, the following lines must be added:

./src/sdk/*<new\_driver>*/src

./src/sdk/*<new\_driver>*/test

Everything contained in those directories will be compiled.

The main test file should contain a test function named: int32\_t new\_driver\_test(void). Hence, when building, the parameter “– new\_driver” can simply be used.

When using the build ALL option, this test can also be added into the function void ALL\_test(void) available in ./src/mx6dq/mx6dq.c.

# Firmware Guide

The i.MX 6 Series Firmware Guide contains detailed documentation of the peripherals supported by the SDK and the associated drivers. The document **IMX6FG\_RevD.pdf** is located in the doc folder of release package.

# Register definitions

Included with the SDK is a full set of register definition C language header files for all modules on the i.MX 6 Series chips. These headers are located under sdk/include/*<chip>*/registers. The macros defined in the header files are generated from the same source material as the register definition sections in the reference manuals and use the same names listed in those sections. In addition, the full documentation of each register and bitfield found in the reference manual is available in the header files as comments.

Further information about the header files can be found in the **Register header quick reference.pdf** file located in the doc directory.

To aid in debugging, the SDK includes complete register definitions for both the ARM RealView Debugger and Lauterbach TRACE32. These files are found under tools/rvd/registers and tools/lauterbach. A PDF describing how to install and use the RealView register definitions is in the doc directory.

# IOMUX Tool

IOMUX Tool helps document and validate the IOMUX configuration for a board. The tool is intended to be used by board designers to generate a design file describing pin mux and pad settings for a board. It can then automatically generate source code (.h and .c files) with functions to setup IOMUXC register configuration. This frees device driver developers from board design details of each pin and pad. The source code generated by the tool is used as-is by the SDK.

The IOMUX Tool executable is available with the release package in the tools/windows/iomux folder. Also included in that directory is the IOMUX Tool manual PDF.

IOMUX design files for all boards supported by the SDK are located under the chip- and board-specific source directories at sdk/*<chip>*/*<board>*/. For instance, the i.MX6DQ SABRE-AI design file is at sdk/mx6dq/sabre\_ai\_rev\_b/i.MX6DQ\_Sabre\_AI\_RevB.IomuxDesign.xml.

# Doxygen

The SDK comes with a Doxygen configuration file and all source code in the SDK is commented with Doxygen-style documentation comments. This means that Doxygen can be used to generate comprehensive documentation for all source files and functions in the SDK.

Install Doxygen by downloading it from:

<http://doxygen.org/>

Doxygen also depends on the Graphviz project to produce graphs.

<http://www.graphviz.org/>

If the Graphviz tool dot is not installed in a directory in your environment PATH, you will need to edit the Doxyfile configuration file and modify the DOT\_PATH setting as appropriate. Doxygen will still run and produce documentation without dot being available, but the output documentation will contain broken image links to graphs.

To generate the SDK source code documentation, simply execute the doxygen command with no arguments from the SDK installation root directory. HTML documentation output will be placed into the doc/html directory. To view the documentation, open doc/html/index.html in a browser:

# Install the video decoding demo

This section described in detail how to setup and run the dual video + dual HD1080P60 display demo on i.MX6 Series EVB / Sabre Lite / Smart Device boards. A single display can optionally be used instead.

Style key for the steps below:

Text for console output.

Text for user input.

***Text for important hints.***

1. How to build the program?

**./tools/build-sdk –t mx6dq –b evb –r vpu –c**

1. How to setup the demo?
2. Create the image over SD card. Under Linux, using fdisk/mkfs.vfat/dd to create a bootable image together with the FAT32 file system on the same SD card.

* sudo fdisk /dev/sdx , sdx is the device name of your SD card.

**sudo fdisk /dev/sdb**

Command (m for help): **m**

***Delete existing partition if there is.***

Command (m for help): **d**

Selected partition 1

Command (m for help): **n**

Command action

e extended

p primary partition (1-4)

**p**

Partition number (1-4): **1**

First cylinder (1-1023, default 1): **256**

***Here the start address should be larger than 2M (space reserved to program the test binary). If one cylinder is 4k, then here 1G is reserved.***

Last cylinder or +size or +sizeM or +sizeK (256-1023, default 1023): **1023**

Command (m for help): w

The partition table has been altered!

Calling ioctl() to re-read partition table.

Syncing disks.

Now there’s one partition on the SD card.

**cat /proc/partitions**

major minor #blocks name

8 0 78125000 sda

8 1 104391 sda1

8 2 78019672 sda2

253 0 75956224 dm-0

253 1 2031616 dm-1

8 16 3872256 sdb

8 17 2904576 sdb1

* Using mkfs.vfat to format the partition:

**sudo mkfs.vfat /dev/sdb1**

* Copy two video clips to the SD card. ***Note that the filename should be less than 8 characters with “.264” extension. The video should be raw H.264 encoded files with no container. The program will find the first two valid .264 files for playing.***
* Burn the image to the SD card.

**sudo dd if=output/mx6dq/evb\_rev\_a/bin/mx6dq\_evb\_rev\_a-vpu-sdk.bin of=/dev/sdb seek=2 skip=2 bs=512 && sync**

***Note that seek=2 skip=2 is mandatory, without them the MBR of the file system will be overwritten.***

1. Put the SD card into SLOT4.
2. Set the boot switch to boot from SD4.
3. Plug the HDMI cable of the first display to J5 of the CPU board.
4. Connect the serial cable for console output and 5V power supply, power on the board.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Diagnostics Suite (1.0) for i.MX6DQ TO1.0 Sabre-Lite Board Rev A

Build: Mar 8 2012, 16:22:20

Freescale Semiconductor, Inc.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

======== Clock frequencies(HZ) =========

Cortex A9 core : 792,000,000

DDR memory : 528,000,000

UART2 for debug : 80,000,000

EPIT1 for system timer : 66,000,000

========================================

========== DDR configuration ===========

data bits: 64, num\_banks: 8

row: 14, col: 10

DDR type is DDR3

Chip select CSD0 is used

Density per chip select: 1024MB

========================================

[INFO] Product Info: i.MX6Q

[INFO] VPU firmware version: 2.1.2

0 - VPU DECODER TEST

1 - VPU ENCODER TEST

x - to exit.

From this prompt, the user is invited to choose what to do.

1. Limitations
2. There is no resizing on the video output. For example if you are decoding some video clips with resolution other than 1080p, the video will show on the top-left of the screen with its original size.
3. Video clips must be raw without container.
4. Currently only H.264 video decoding is supported. Other formats such as VC1, H.263, MPEG3, MPEG4 may be added in a future release.

# Known limitations

These are the current set of known bugs and issues in the Platform SDK.

* The TEMPMON driver over-temperature alarm feature does not work.
* The GPMI NAND driver API calls to read and write NAND pages with BCH ECC do not work correctly.
* The CCM driver (ccm\_pll.c) does not support getting clocks for all peripherals from its get\_peri\_clock() API.